|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **PURCHASE ORDER** | | |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Po no: 23-24 Multi Bath 312 | | |  |  |  | Date: 06/11/2023 | |  |
| Supplier Multi Bath Service | | | |  |  | Quotation: Email | | |
| Billing Address: 114, Gera Imperium Green, Next to | | | | | |  | |  |
|  |  | Jairam complex, Mala Panaji Goa 403001 | | |  |  | | |
| Shipping Address: : Flat No – C 801, Edcon Rio Grande | | | | | |  | |  |
|  |  | Campal Panaji Goa403001 | | | |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No** | **Item Description** | **QTY** | **Pricing Per Unit** | **Total** |
| 1 | **Jacuzzi Massage Bath Tub** | 1 | 139830.5 | 139831 |
| Jacuzzi system with 6 hydrojets Body Jet big |
| Whirlpool Motor 1.5 HP |
| Fully Body Stand SS 316 |
| Pop Drainage System |
| Bubble bath with 24 jet Supported air blower |
| 12 Micro jets |
| Spinal Massager Jet 12 PCS 4 foot massager 8 back massager |
| Bubble blower 0.5hp |
| Multicolour 2 Led light chromatography 7 colour change |
| Designer Headrest pillow 2 psc |
| Full Water Capacity |
| Jacuzzi ON/OFF push button speed controller regulator |
| Bubble ON/OFF push button |
| Fully computerized control panel |
| Filler set hot cold and mixture diverter spout hand shower 3 flow system |
| Touch screen with control panel |
| Water level controller |
| Stereo phonic radio FM |
| Bluetooth & aux music system |
| Automatic Shut |
| Earth leakage circuit breaker |
| Suction unit |
| Self draining pipes |
| Ozonizer |
| wooden frem |
| online heater |
| Size 6\*5\*2fit |
| 2 | **S S Steam Generator** | 1 | 16949.1 | 16949.1 |
| SS outer body |
| SS 316 Water tank |
| Digital control panel operated |
| Auto time cut off​ system |
| Safety value brush |
| Drain value brush |
| Soil noise value |
| Steam head |
| Time and​ temperature control |
| Digital control |
| Aoto tampreture cut off system |
| Auto draining​ system |
| Stainless steel 304 grade 16 grade steam tank |
| Stainless steel make heating element​ for long life |
| 26mm thickness PUF insolution |
| DRP for heating element |
| Water level sensor​ cut off to ensure heater safety |
| Safety pressure relise value |
| Flexible house connector for​ water fidding |
| Steam diff user outlet |
| Soft touch swithess |
| LED display panel |
| Stainless​ steel socket for long life |
| Short circuit protection |
| High current protection |
| Earth leakage Steam generator 6kw |
| **Total** | | | | **156780** |
| **GST 18%** | | | | **28220.3** |
| **Grand Total** | | | | **185000** |

**Payment Terms**

50% Advance

Balance on Delivery

**Warranty Terms**

5 years warranty on motor

10 years warranty on tub

2 years warranty on rest

Terms and conditions apply as per norms JPT001

Kindly dispatch the material as per quotation mentioned

Payment after receipt of material